ALFER connector type AC1 consists of a single steel body composed of UNI 5737 M12 × 1.5 × 20 self-tapping thread for mechanical connection to the steel profile, limit-stop and characteristic grooves specifically designed to connect to the concrete of the slab.