Dry connector consisting of a single steel body with a 16 mm diameter, shaped for mechanical hooking between timber and concrete. It is threaded with a continuous screw pitch 6 R3 composed of an external spiral with constant diameter and the internal tapered thread is conical with reverse adaptation. The intermediate part is without thread (maximum shear position) with stop limit and characteristic grooves specifically designed to connect to the concrete of the slab.